Speedup factor S=10  
Efficiency e= 80%= 0.8  
Efficiency e= (Speedup factor s)/(Number of stages k)⎝ e= S/k  
From this k= S/e   
K=S/e=10/0.8=12.5 ͌ 13 stages