**Answer:** **(A)**   
  
**Explanation:** MUX has 8 states bits as input lines so we require 3 select inputs to select and input lines.

No. of bits in control memory next address field=26-13-3 =10

10 bit addressing .we have 2 10 memory size

So X,Y size=10,3

So (A) is correct option.